### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:14.5 (WebPack) - P.58f | Target Family: | Spartan6
OS Platform: | NT | Target Device: | xc6slx9
Project ID (random number) | 44d086c375374309a4c0e33b48910796.94c360dfdef74d669d5eb6ea67e85822.1 | Target Package: | tqg144
Registration ID | __0_0_0 | Target Speed: | -3
Date Generated | 2015-11-13T16:25:40 | Tool Flow | CommandLine

User Environment
OS Name | Microsoft Windows XP Professional | OS Release | Service Pack 3 (build 2600)
CPU Name | AMD Phenom(tm) 9650 Quad-Core Processor | CPU Speed | 2310 MHz
OS Name | Microsoft Windows XP Professional | OS Release | Service Pack 3 (build 2600)
CPU Name | AMD Phenom(tm) 9650 Quad-Core Processor | CPU Speed | 2310 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
| MiscellaneousStatistics AGG_BONDED_IO=11 AGG_IO=11 AGG_LOCED_IO=11 AGG_SLICE=723 NUM_BONDED_IOB=11 NUM_BSCAN=1 NUM_BSFULL=887 NUM_BSLUTONLY=808 NUM_BSREGONLY=410 NUM_BSUSED=2105 NUM_BUFG=2 NUM_BUFIO2=1 NUM_DPRAM_O5ANDO6=64 NUM_DSP48A1=3 NUM_IOB_FF=8 NUM_LOCED_IOB=11 NUM_LOGIC_O5ANDO6=268 NUM_LOGIC_O5ONLY=42 NUM_LOGIC_O6ONLY=1213 NUM_LUT_RT_DRIVES_CARRY4=3 NUM_LUT_RT_DRIVES_FLOP=34 NUM_LUT_RT_EXO5=34 NUM_LUT_RT_EXO6=1 NUM_LUT_RT_O5=9 NUM_LUT_RT_O5ANDO6=2 NUM_LUT_RT_O6=41 NUM_OLOGIC2=8 NUM_PLL_ADV=1 NUM_RAMB16BWER=4 NUM_SLICEL=164 NUM_SLICEM=43 NUM_SLICEX=516 NUM_SLICE_CARRY4=51 NUM_SLICE_CONTROLSET=98 NUM_SLICE_CYINIT=2139 NUM_SLICE_F7MUX=118 NUM_SLICE_FF=1387 NUM_SLICE_LATCHLOGIC=7 NUM_SLICE_UNUSEDCTRL=72 NUM_SRL_O5ANDO6=50 NUM_SRL_O5ONLY=1 NUM_SRL_O6ONLY=20 NUM_UNUSABLE_FF_BELS=404 Xilinx Core clock_generator_v4_03_a=1 Xilinx Core lmb_bram_elaborate_v1_00_a=1 Xilinx Core lmb_bram_if_cntlr_v3_10_c=2 Xilinx Core lmb_v10_v2_00_b=2 Xilinx Core mdm_v2_10_a=1 Xilinx Core microblaze_v8_50_a=1 Xilinx Core plb_v46_v1_05_a=1 Xilinx Core proc_sys_reset_v3_00_a=1 Xilinx Core xps_gpio_v2_00_a=2 | NetStatistics NumNets_Active=2818 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_BOUNCEACROSS=102 NumNodesOfType_Active_BOUNCEIN=464 NumNodesOfType_Active_BUFGOUT=2 NumNodesOfType_Active_BUFHINP2OUT=15 NumNodesOfType_Active_BUFIOINP=1 NumNodesOfType_Active_CLKPIN=659 NumNodesOfType_Active_CLKPINFEED=22 NumNodesOfType_Active_CNTRLPIN=857 NumNodesOfType_Active_DOUBLE=5413 NumNodesOfType_Active_GENERIC=14 NumNodesOfType_Active_GLOBAL=140 NumNodesOfType_Active_INPUT=513 NumNodesOfType_Active_IOBIN2OUT=10 NumNodesOfType_Active_IOBOUTPUT=10 NumNodesOfType_Active_LUTINPUT=7543 NumNodesOfType_Active_OUTBOUND=2891 NumNodesOfType_Active_OUTPUT=2903 NumNodesOfType_Active_PADINPUT=8 NumNodesOfType_Active_PADOUTPUT=3 NumNodesOfType_Active_PINBOUNCE=2185 NumNodesOfType_Active_PINFEED=8997 NumNodesOfType_Active_PINFEED2=8 NumNodesOfType_Active_QUAD=3387 NumNodesOfType_Active_REGINPUT=766 NumNodesOfType_Active_SINGLE=6069 NumNodesOfType_Gnd_BOUNCEACROSS=2 NumNodesOfType_Gnd_BOUNCEIN=105 NumNodesOfType_Gnd_CLKPIN=1 NumNodesOfType_Gnd_CNTRLPIN=7 NumNodesOfType_Gnd_DOUBLE=11 NumNodesOfType_Gnd_HGNDOUT=53 NumNodesOfType_Gnd_INPUT=565 NumNodesOfType_Gnd_LUTINPUT=92 NumNodesOfType_Gnd_OUTBOUND=30 NumNodesOfType_Gnd_OUTPUT=42 NumNodesOfType_Gnd_PINBOUNCE=231 NumNodesOfType_Gnd_PINFEED=581 NumNodesOfType_Gnd_REGINPUT=28 NumNodesOfType_Gnd_SINGLE=26 NumNodesOfType_Vcc_CLKPIN=5 NumNodesOfType_Vcc_CNTRLPIN=11 NumNodesOfType_Vcc_HVCCOUT=191 NumNodesOfType_Vcc_INPUT=7 NumNodesOfType_Vcc_KVCCOUT=36 NumNodesOfType_Vcc_LUTINPUT=508 NumNodesOfType_Vcc_PINBOUNCE=15 NumNodesOfType_Vcc_PINFEED=519 NumNodesOfType_Vcc_REGINPUT=3 SiteStatistics BUFG-BUFGMUX=2 IOB-IOBM=7 IOB-IOBS=4 SLICEL-SLICEM=89 SLICEX-SLICEL=109 SLICEX-SLICEM=83 | SiteSummary BSCAN=1 BSCAN_BSCAN=1 BUFG=2 BUFG_BUFG=2 BUFIO2=1 BUFIO2_BUFIO2=1 CARRY4=51 DSP48A1=3 DSP48A1_DSP48A1=3 FF_SR=106 HARD0=4 HARD1=6 IOB=11 IOB_IMUX=3 IOB_INBUF=3 IOB_OUTBUF=8 LUT5=352 LUT6=1518 LUT_OR_MEM5=118 LUT_OR_MEM6=141 OLOGIC2=8 OLOGIC2_OUTFF=8 PAD=11 PLL_ADV=1 PLL_ADV_PLL_ADV=1 PULL_OR_KEEP1=8 RAMB16BWER=4 RAMB16BWER_RAMB16BWER=4 REG_SR=1288 SELMUX2_1=118 SLICEL=164 SLICEM=43 SLICEX=516

Configuration Data
BSCAN_BSCAN JTAG_CHAIN=[2:1] JTAG_TEST=[0:1] BUFIO2_BUFIO2 DIVIDE=[1:1] DIVIDE_BYPASS=[TRUE:1] I_INVERT=[FALSE:1] DSP48A1 CEA=[CEA_INV:0] [CEA:3] CEB=[CEB_INV:0] [CEB:3] CEC=[CEC:3] [CEC_INV:0] CECARRYIN=[CECARRYIN:3] [CECARRYIN_INV:0] CED=[CED_INV:0] [CED:3] CEM=[CEM_INV:0] [CEM:3] CEOPMODE=[CEOPMODE_INV:0] [CEOPMODE:3] CEP=[CEP:3] [CEP_INV:0] CLK=[CLK:3] [CLK_INV:0] RSTA=[RSTA:3] [RSTA_INV:0] RSTB=[RSTB:3] [RSTB_INV:0] RSTC=[RSTC_INV:0] [RSTC:3] RSTCARRYIN=[RSTCARRYIN_INV:0] [RSTCARRYIN:3] RSTD=[RSTD_INV:0] [RSTD:3] RSTM=[RSTM:3] [RSTM_INV:0] RSTOPMODE=[RSTOPMODE_INV:0] [RSTOPMODE:3] RSTP=[RSTP_INV:0] [RSTP:3] DSP48A1_DSP48A1 A0REG=[0:2] [1:1] A1REG=[0:3] B0REG=[0:2] [1:1] B1REG=[0:3] B_INPUT=[DIRECT:3] CARRYINREG=[0:3] CARRYINSEL=[OPMODE5:3] CARRYOUTREG=[0:3] CEA=[CEA_INV:0] [CEA:3] CEB=[CEB_INV:0] [CEB:3] CEC=[CEC:3] [CEC_INV:0] CECARRYIN=[CECARRYIN:3] [CECARRYIN_INV:0] CED=[CED_INV:0] [CED:3] CEM=[CEM_INV:0] [CEM:3] CEOPMODE=[CEOPMODE_INV:0] [CEOPMODE:3] CEP=[CEP:3] [CEP_INV:0] CLK=[CLK:3] [CLK_INV:0] CREG=[0:3] DREG=[0:3] MREG=[0:1] [1:2] OPMODEREG=[0:3] PREG=[0:1] [1:2] RSTA=[RSTA:3] [RSTA_INV:0] RSTB=[RSTB:3] [RSTB_INV:0] RSTC=[RSTC_INV:0] [RSTC:3] RSTCARRYIN=[RSTCARRYIN_INV:0] [RSTCARRYIN:3] RSTD=[RSTD_INV:0] [RSTD:3] RSTM=[RSTM:3] [RSTM_INV:0] RSTOPMODE=[RSTOPMODE_INV:0] [RSTOPMODE:3] RSTP=[RSTP_INV:0] [RSTP:3] RSTTYPE=[SYNC:3] | FF_SR CK=[CK:106] [CK_INV:0] SRINIT=[SRINIT0:99] [SRINIT1:7] SYNC_ATTR=[ASYNC:29] [SYNC:77] IOB_OUTBUF DRIVEATTRBOX=[2:8] SLEW=[SLOW:8] SUSPEND=[3STATE:8] LUT_OR_MEM5 CLK=[CLK:115] [CLK_INV:0] LUT_OR_MEM=[LUT:3] [RAM:115] RAMMODE=[SRL16:51] [DPRAM32:64] LUT_OR_MEM6 CLK=[CLK:134] [CLK_INV:0] LUT_OR_MEM=[LUT:7] [RAM:134] RAMMODE=[SRL16:70] [DPRAM32:64] OLOGIC2 CLK0=[CLK0_INV:0] [CLK0:8] OLOGIC2_OUTFF CK0=[CK0_INV:0] [CK0:8] OUTFFTYPE=[FF:8] SRINIT_OQ=[0:8] SRTYPE_OQ=[SYNC:8] PLL_ADV RST=[RST:0] [RST_INV:1] PLL_ADV_PLL_ADV BANDWIDTH=[OPTIMIZED:1] CLK_FEEDBACK=[CLKFBOUT:1] COMPENSATION=[INTERNAL:1] PLL_ADD_LEAKAGE=[2:1] PLL_AVDD_COMP_SET=[2:1] PLL_CLAMP_BYPASS=[FALSE:1] PLL_CLAMP_REF_SEL=[1:1] PLL_CLK0MX=[0:1] PLL_CLK1MX=[0:1] PLL_CLK2MX=[0:1] PLL_CLK3MX=[0:1] PLL_CLK4MX=[0:1] PLL_CLK5MX=[0:1] PLL_CLKBURST_CNT=[0:1] PLL_CLKBURST_ENABLE=[TRUE:1] PLL_CLKCNTRL=[0:1] PLL_CLKFBMX=[0:1] PLL_CLKFBOUT2_EDGE=[TRUE:1] PLL_CLKFBOUT2_NOCOUNT=[TRUE:1] PLL_CLKFBOUT_EDGE=[TRUE:1] PLL_CLKFBOUT_EN=[FALSE:1] PLL_CLKFBOUT_NOCOUNT=[TRUE:1] PLL_CLKOUT0_EDGE=[TRUE:1] PLL_CLKOUT0_EN=[FALSE:1] PLL_CLKOUT0_NOCOUNT=[TRUE:1] PLL_CLKOUT1_EDGE=[TRUE:1] PLL_CLKOUT1_EN=[FALSE:1] PLL_CLKOUT1_NOCOUNT=[TRUE:1] PLL_CLKOUT2_EDGE=[TRUE:1] PLL_CLKOUT2_EN=[FALSE:1] PLL_CLKOUT2_NOCOUNT=[TRUE:1] PLL_CLKOUT3_EDGE=[TRUE:1] PLL_CLKOUT3_EN=[FALSE:1] PLL_CLKOUT3_NOCOUNT=[TRUE:1] PLL_CLKOUT4_EDGE=[TRUE:1] PLL_CLKOUT4_EN=[FALSE:1] PLL_CLKOUT4_NOCOUNT=[TRUE:1] PLL_CLKOUT5_EDGE=[TRUE:1] PLL_CLKOUT5_EN=[FALSE:1] PLL_CLKOUT5_NOCOUNT=[TRUE:1] PLL_CLK_LOST_DETECT=[FALSE:1] PLL_CP=[1:1] PLL_CP_BIAS_TRIP_SHIFT=[TRUE:1] PLL_CP_REPL=[1:1] PLL_CP_RES=[0:1] PLL_DIRECT_PATH_CNTRL=[TRUE:1] PLL_DIVCLK_EDGE=[TRUE:1] PLL_DIVCLK_NOCOUNT=[TRUE:1] PLL_DVDD_COMP_SET=[2:1] PLL_EN=[FALSE:1] PLL_EN_DLY=[TRUE:1] PLL_EN_LEAKAGE=[2:1] PLL_EN_TCLK0=[TRUE:1] PLL_EN_TCLK1=[TRUE:1] PLL_EN_TCLK2=[TRUE:1] PLL_EN_TCLK3=[TRUE:1] PLL_EN_VCO0=[FALSE:1] PLL_EN_VCO1=[FALSE:1] PLL_EN_VCO2=[FALSE:1] PLL_EN_VCO3=[FALSE:1] PLL_EN_VCO4=[FALSE:1] PLL_EN_VCO5=[FALSE:1] PLL_EN_VCO6=[FALSE:1] PLL_EN_VCO7=[FALSE:1] PLL_EN_VCO_DIV1=[FALSE:1] PLL_EN_VCO_DIV6=[TRUE:1] PLL_INTFB=[0:1] PLL_IO_CLKSRC=[0:1] PLL_LFHF=[3:1] PLL_LOCK_FB_DLY=[3:1] PLL_LOCK_REF_DLY=[5:1] PLL_MAN_LF_EN=[TRUE:1] PLL_NBTI_EN=[TRUE:1] PLL_PFD_CNTRL=[8:1] PLL_PFD_DLY=[1:1] PLL_PWRD_CFG=[FALSE:1] PLL_REG_INPUT=[TRUE:1] PLL_RES=[1:1] PLL_SEL_SLIPD=[FALSE:1] PLL_SKEW_CNTRL=[0:1] PLL_TEST_IN_WINDOW=[FALSE:1] PLL_VDD_SEL=[0:1] PLL_VLFHIGH_DIS=[TRUE:1] RST=[RST:0] [RST_INV:1] | PULL_OR_KEEP1 PULLTYPE=[PULLUP:8] RAMB16BWER CLKA=[CLKA_INV:0] [CLKA:4] CLKB=[CLKB_INV:0] [CLKB:4] ENA=[ENA_INV:0] [ENA:4] ENB=[ENB_INV:0] [ENB:4] REGCEA=[REGCEA_INV:0] [REGCEA:4] REGCEB=[REGCEB_INV:0] [REGCEB:4] RSTA=[RSTA:4] [RSTA_INV:0] RSTB=[RSTB:4] [RSTB_INV:0] WEA0=[WEA0:4] [WEA0_INV:0] WEA1=[WEA1:4] [WEA1_INV:0] WEA2=[WEA2:4] [WEA2_INV:0] WEA3=[WEA3_INV:0] [WEA3:4] WEB0=[WEB0:4] [WEB0_INV:0] WEB1=[WEB1:4] [WEB1_INV:0] WEB2=[WEB2_INV:0] [WEB2:4] WEB3=[WEB3:4] [WEB3_INV:0] RAMB16BWER_RAMB16BWER CLKA=[CLKA_INV:0] [CLKA:4] CLKB=[CLKB_INV:0] [CLKB:4] DATA_WIDTH_A=[9:4] DATA_WIDTH_B=[9:4] DOA_REG=[0:4] DOB_REG=[0:4] ENA=[ENA_INV:0] [ENA:4] ENB=[ENB_INV:0] [ENB:4] EN_RSTRAM_A=[TRUE:4] EN_RSTRAM_B=[TRUE:4] RAM_MODE=[TDP:4] REGCEA=[REGCEA_INV:0] [REGCEA:4] REGCEB=[REGCEB_INV:0] [REGCEB:4] RSTA=[RSTA:4] [RSTA_INV:0] RSTB=[RSTB:4] [RSTB_INV:0] RSTTYPE=[SYNC:4] RST_PRIORITY_A=[CE:4] RST_PRIORITY_B=[CE:4] WEA0=[WEA0:4] [WEA0_INV:0] WEA1=[WEA1:4] [WEA1_INV:0] WEA2=[WEA2:4] [WEA2_INV:0] WEA3=[WEA3_INV:0] [WEA3:4] WEB0=[WEB0:4] [WEB0_INV:0] WEB1=[WEB1:4] [WEB1_INV:0] WEB2=[WEB2_INV:0] [WEB2:4] WEB3=[WEB3:4] [WEB3_INV:0] WRITE_MODE_A=[WRITE_FIRST:4] WRITE_MODE_B=[WRITE_FIRST:4] REG_SR CK=[CK:1267] [CK_INV:21] LATCH_OR_FF=[FF:1281] [AND2L:7] SRINIT=[SRINIT0:1210] [SRINIT1:78] SYNC_ATTR=[ASYNC:352] [SYNC:936] SLICEL CLK=[CLK:138] [CLK_INV:5] SLICEM CLK=[CLK:43] [CLK_INV:0] | SLICEX CLK=[CLK:460] [CLK_INV:5]

Pin Data
BSCAN CAPTURE=1 DRCK=1 SEL=1 SHIFT=1 TDI=1 TDO=1 UPDATE=1 BSCAN_BSCAN CAPTURE=1 DRCK=1 SEL=1 SHIFT=1 TDI=1 TDO=1 UPDATE=1 BUFG I0=2 O=2 BUFG_BUFG I0=2 O=2 BUFIO2 DIVCLK=1 I=1 BUFIO2_BUFIO2 DIVCLK=1 I=1 CARRY4 CIN=35 CO0=3 CO1=3 CO2=7 CO3=40 CYINIT=16 DI0=46 DI1=41 DI2=40 DI3=37 O0=27 O1=28 O2=27 O3=28 S0=51 S1=46 S2=45 S3=43 DSP48A1 A0=3 A1=3 A10=3 A11=3 A12=3 A13=3 A14=3 A15=3 A16=3 A17=3 A2=3 A3=3 A4=3 A5=3 A6=3 A7=3 A8=3 A9=3 B0=3 B1=3 B10=3 B11=3 B12=3 B13=3 B14=3 B15=3 B16=3 B17=3 B2=3 B3=3 B4=3 B5=3 B6=3 B7=3 B8=3 B9=3 C0=3 C1=3 C10=3 C11=3 C12=3 C13=3 C14=3 C15=3 C16=3 C17=3 C18=3 C19=3 C2=3 C20=3 C21=3 C22=3 C23=3 C24=3 C25=3 C26=3 C27=3 C28=3 C29=3 C3=3 C30=3 C31=3 C32=3 C33=3 C34=3 C35=3 C36=3 C37=3 C38=3 C39=3 C4=3 C40=3 C41=3 C42=3 C43=3 C44=3 C45=3 C46=3 C47=3 C5=3 C6=3 C7=3 C8=3 C9=3 CEA=3 CEB=3 CEC=3 CECARRYIN=3 CED=3 CEM=3 CEOPMODE=3 CEP=3 CLK=3 D0=3 D1=3 D10=3 D11=3 D12=3 D13=3 D14=3 D15=3 D16=3 D17=3 D2=3 D3=3 D4=3 D5=3 D6=3 D7=3 D8=3 D9=3 OPMODE0=3 OPMODE1=3 OPMODE2=3 OPMODE3=3 OPMODE4=3 OPMODE5=3 OPMODE6=3 OPMODE7=3 P0=2 P1=2 P10=2 P11=2 P12=2 P13=2 P14=2 P15=1 P16=1 P17=1 P18=1 P19=1 P2=2 P20=1 P21=1 P22=1 P23=1 P24=1 P25=1 P26=1 P27=1 P28=1 P29=1 P3=2 P30=1 P31=1 P32=1 P33=1 P34=1 P35=1 P36=1 P37=1 P38=1 P39=1 P4=2 P40=1 P41=1 P42=1 P43=1 P44=1 P45=1 P46=1 P47=1 P5=2 P6=2 P7=2 P8=2 P9=2 PCIN0=1 PCIN1=1 PCIN10=1 PCIN11=1 PCIN12=1 PCIN13=1 PCIN14=1 PCIN15=1 PCIN16=1 PCIN17=1 PCIN18=1 PCIN19=1 PCIN2=1 PCIN20=1 PCIN21=1 PCIN22=1 PCIN23=1 PCIN24=1 PCIN25=1 PCIN26=1 PCIN27=1 PCIN28=1 PCIN29=1 PCIN3=1 PCIN30=1 PCIN31=1 PCIN32=1 PCIN33=1 PCIN34=1 PCIN35=1 PCIN36=1 PCIN37=1 PCIN38=1 PCIN39=1 PCIN4=1 PCIN40=1 PCIN41=1 PCIN42=1 PCIN43=1 PCIN44=1 PCIN45=1 PCIN46=1 PCIN47=1 PCIN5=1 PCIN6=1 PCIN7=1 PCIN8=1 PCIN9=1 PCOUT0=1 PCOUT1=1 PCOUT10=1 PCOUT11=1 PCOUT12=1 PCOUT13=1 PCOUT14=1 PCOUT15=1 PCOUT16=1 PCOUT17=1 PCOUT18=1 PCOUT19=1 PCOUT2=1 PCOUT20=1 PCOUT21=1 PCOUT22=1 PCOUT23=1 PCOUT24=1 PCOUT25=1 PCOUT26=1 PCOUT27=1 PCOUT28=1 PCOUT29=1 PCOUT3=1 PCOUT30=1 PCOUT31=1 PCOUT32=1 PCOUT33=1 PCOUT34=1 PCOUT35=1 PCOUT36=1 PCOUT37=1 PCOUT38=1 PCOUT39=1 PCOUT4=1 PCOUT40=1 PCOUT41=1 PCOUT42=1 PCOUT43=1 PCOUT44=1 PCOUT45=1 PCOUT46=1 PCOUT47=1 PCOUT5=1 PCOUT6=1 PCOUT7=1 PCOUT8=1 PCOUT9=1 RSTA=3 RSTB=3 RSTC=3 RSTCARRYIN=3 RSTD=3 RSTM=3 RSTOPMODE=3 RSTP=3 | DSP48A1_DSP48A1 A0=3 A1=3 A10=3 A11=3 A12=3 A13=3 A14=3 A15=3 A16=3 A17=3 A2=3 A3=3 A4=3 A5=3 A6=3 A7=3 A8=3 A9=3 B0=3 B1=3 B10=3 B11=3 B12=3 B13=3 B14=3 B15=3 B16=3 B17=3 B2=3 B3=3 B4=3 B5=3 B6=3 B7=3 B8=3 B9=3 C0=3 C1=3 C10=3 C11=3 C12=3 C13=3 C14=3 C15=3 C16=3 C17=3 C18=3 C19=3 C2=3 C20=3 C21=3 C22=3 C23=3 C24=3 C25=3 C26=3 C27=3 C28=3 C29=3 C3=3 C30=3 C31=3 C32=3 C33=3 C34=3 C35=3 C36=3 C37=3 C38=3 C39=3 C4=3 C40=3 C41=3 C42=3 C43=3 C44=3 C45=3 C46=3 C47=3 C5=3 C6=3 C7=3 C8=3 C9=3 CEA=3 CEB=3 CEC=3 CECARRYIN=3 CED=3 CEM=3 CEOPMODE=3 CEP=3 CLK=3 D0=3 D1=3 D10=3 D11=3 D12=3 D13=3 D14=3 D15=3 D16=3 D17=3 D2=3 D3=3 D4=3 D5=3 D6=3 D7=3 D8=3 D9=3 OPMODE0=3 OPMODE1=3 OPMODE2=3 OPMODE3=3 OPMODE4=3 OPMODE5=3 OPMODE6=3 OPMODE7=3 P0=2 P1=2 P10=2 P11=2 P12=2 P13=2 P14=2 P15=1 P16=1 P17=1 P18=1 P19=1 P2=2 P20=1 P21=1 P22=1 P23=1 P24=1 P25=1 P26=1 P27=1 P28=1 P29=1 P3=2 P30=1 P31=1 P32=1 P33=1 P34=1 P35=1 P36=1 P37=1 P38=1 P39=1 P4=2 P40=1 P41=1 P42=1 P43=1 P44=1 P45=1 P46=1 P47=1 P5=2 P6=2 P7=2 P8=2 P9=2 PCIN0=1 PCIN1=1 PCIN10=1 PCIN11=1 PCIN12=1 PCIN13=1 PCIN14=1 PCIN15=1 PCIN16=1 PCIN17=1 PCIN18=1 PCIN19=1 PCIN2=1 PCIN20=1 PCIN21=1 PCIN22=1 PCIN23=1 PCIN24=1 PCIN25=1 PCIN26=1 PCIN27=1 PCIN28=1 PCIN29=1 PCIN3=1 PCIN30=1 PCIN31=1 PCIN32=1 PCIN33=1 PCIN34=1 PCIN35=1 PCIN36=1 PCIN37=1 PCIN38=1 PCIN39=1 PCIN4=1 PCIN40=1 PCIN41=1 PCIN42=1 PCIN43=1 PCIN44=1 PCIN45=1 PCIN46=1 PCIN47=1 PCIN5=1 PCIN6=1 PCIN7=1 PCIN8=1 PCIN9=1 PCOUT0=1 PCOUT1=1 PCOUT10=1 PCOUT11=1 PCOUT12=1 PCOUT13=1 PCOUT14=1 PCOUT15=1 PCOUT16=1 PCOUT17=1 PCOUT18=1 PCOUT19=1 PCOUT2=1 PCOUT20=1 PCOUT21=1 PCOUT22=1 PCOUT23=1 PCOUT24=1 PCOUT25=1 PCOUT26=1 PCOUT27=1 PCOUT28=1 PCOUT29=1 PCOUT3=1 PCOUT30=1 PCOUT31=1 PCOUT32=1 PCOUT33=1 PCOUT34=1 PCOUT35=1 PCOUT36=1 PCOUT37=1 PCOUT38=1 PCOUT39=1 PCOUT4=1 PCOUT40=1 PCOUT41=1 PCOUT42=1 PCOUT43=1 PCOUT44=1 PCOUT45=1 PCOUT46=1 PCOUT47=1 PCOUT5=1 PCOUT6=1 PCOUT7=1 PCOUT8=1 PCOUT9=1 RSTA=3 RSTB=3 RSTC=3 RSTCARRYIN=3 RSTD=3 RSTM=3 RSTOPMODE=3 RSTP=3 FF_SR CE=48 CK=106 D=106 Q=106 SR=88 HARD0 0=4 HARD1 1=6 IOB I=3 O=8 PAD=11 | IOB_IMUX I=3 OUT=3 IOB_INBUF OUT=3 PAD=3 IOB_OUTBUF IN=8 OUT=8 LUT5 A1=145 A2=197 A3=174 A4=142 A5=168 O5=352 LUT6 A1=589 A2=881 A3=1173 A4=1375 A5=1477 A6=1496 O6=1518 LUT_OR_MEM5 A1=115 A2=115 A3=115 A4=115 A5=115 CLK=115 DI1=115 O5=118 WA1=64 WA2=64 WA3=64 WA4=64 WA5=64 WE=115 LUT_OR_MEM6 A1=135 A2=136 A3=137 A4=138 A5=141 A6=141 CLK=134 DI2=134 MC31=7 O6=125 WA1=64 WA2=64 WA3=64 WA4=64 WA5=64 WA6=64 WE=134 OLOGIC2 CLK0=8 D1=8 OCE=8 OQ=8 SR=8 OLOGIC2_OUTFF CE=8 CK0=8 D1=8 Q=8 SR=8 PAD PAD=11 PLL_ADV CLKFBIN=1 CLKFBOUT=1 CLKIN1=1 CLKOUT0=1 DADDR0=1 DADDR1=1 DADDR2=1 DADDR3=1 DADDR4=1 DCLK=1 DEN=1 DI0=1 DI1=1 DI10=1 DI11=1 DI12=1 DI13=1 DI14=1 DI15=1 DI2=1 DI3=1 DI4=1 DI5=1 DI6=1 DI7=1 DI8=1 DI9=1 DWE=1 LOCKED=1 RST=1 PLL_ADV_PLL_ADV CLKFBIN=1 CLKFBOUT=1 CLKIN1=1 CLKOUT0=1 DADDR0=1 DADDR1=1 DADDR2=1 DADDR3=1 DADDR4=1 DCLK=1 DEN=1 DI0=1 DI1=1 DI10=1 DI11=1 DI12=1 DI13=1 DI14=1 DI15=1 DI2=1 DI3=1 DI4=1 DI5=1 DI6=1 DI7=1 DI8=1 DI9=1 DWE=1 LOCKED=1 RST=1 PULL_OR_KEEP1 PAD=8 RAMB16BWER ADDRA0=4 ADDRA1=4 ADDRA10=4 ADDRA11=4 ADDRA12=4 ADDRA13=4 ADDRA2=4 ADDRA3=4 ADDRA4=4 ADDRA5=4 ADDRA6=4 ADDRA7=4 ADDRA8=4 ADDRA9=4 ADDRB0=4 ADDRB1=4 ADDRB10=4 ADDRB11=4 ADDRB12=4 ADDRB13=4 ADDRB2=4 ADDRB3=4 ADDRB4=4 ADDRB5=4 ADDRB6=4 ADDRB7=4 ADDRB8=4 ADDRB9=4 CLKA=4 CLKB=4 DIA0=4 DIA1=4 DIA10=4 DIA11=4 DIA12=4 DIA13=4 DIA14=4 DIA15=4 DIA16=4 DIA17=4 DIA18=4 DIA19=4 DIA2=4 DIA20=4 DIA21=4 DIA22=4 DIA23=4 DIA24=4 DIA25=4 DIA26=4 DIA27=4 DIA28=4 DIA29=4 DIA3=4 DIA30=4 DIA31=4 DIA4=4 DIA5=4 DIA6=4 DIA7=4 DIA8=4 DIA9=4 DIB0=4 DIB1=4 DIB10=4 DIB11=4 DIB12=4 DIB13=4 DIB14=4 DIB15=4 DIB16=4 DIB17=4 DIB18=4 DIB19=4 DIB2=4 DIB20=4 DIB21=4 DIB22=4 DIB23=4 DIB24=4 DIB25=4 DIB26=4 DIB27=4 DIB28=4 DIB29=4 DIB3=4 DIB30=4 DIB31=4 DIB4=4 DIB5=4 DIB6=4 DIB7=4 DIB8=4 DIB9=4 DIPA0=4 DIPA1=4 DIPA2=4 DIPA3=4 DIPB0=4 DIPB1=4 DIPB2=4 DIPB3=4 DOA0=4 DOA1=4 DOA2=4 DOA3=4 DOA4=4 DOA5=4 DOA6=4 DOA7=4 DOB0=4 DOB1=4 DOB2=4 DOB3=4 DOB4=4 DOB5=4 DOB6=4 DOB7=4 ENA=4 ENB=4 REGCEA=4 REGCEB=4 RSTA=4 RSTB=4 WEA0=4 WEA1=4 WEA2=4 WEA3=4 WEB0=4 WEB1=4 WEB2=4 WEB3=4 RAMB16BWER_RAMB16BWER ADDRA0=4 ADDRA1=4 ADDRA10=4 ADDRA11=4 ADDRA12=4 ADDRA13=4 ADDRA2=4 ADDRA3=4 ADDRA4=4 ADDRA5=4 ADDRA6=4 ADDRA7=4 ADDRA8=4 ADDRA9=4 ADDRB0=4 ADDRB1=4 ADDRB10=4 ADDRB11=4 ADDRB12=4 ADDRB13=4 ADDRB2=4 ADDRB3=4 ADDRB4=4 ADDRB5=4 ADDRB6=4 ADDRB7=4 ADDRB8=4 ADDRB9=4 CLKA=4 CLKB=4 DIA0=4 DIA1=4 DIA10=4 DIA11=4 DIA12=4 DIA13=4 DIA14=4 DIA15=4 DIA16=4 DIA17=4 DIA18=4 DIA19=4 DIA2=4 DIA20=4 DIA21=4 DIA22=4 DIA23=4 DIA24=4 DIA25=4 DIA26=4 DIA27=4 DIA28=4 DIA29=4 DIA3=4 DIA30=4 DIA31=4 DIA4=4 DIA5=4 DIA6=4 DIA7=4 DIA8=4 DIA9=4 DIB0=4 DIB1=4 DIB10=4 DIB11=4 DIB12=4 DIB13=4 DIB14=4 DIB15=4 DIB16=4 DIB17=4 DIB18=4 DIB19=4 DIB2=4 DIB20=4 DIB21=4 DIB22=4 DIB23=4 DIB24=4 DIB25=4 DIB26=4 DIB27=4 DIB28=4 DIB29=4 DIB3=4 DIB30=4 DIB31=4 DIB4=4 DIB5=4 DIB6=4 DIB7=4 DIB8=4 DIB9=4 DIPA0=4 DIPA1=4 DIPA2=4 DIPA3=4 DIPB0=4 DIPB1=4 DIPB2=4 DIPB3=4 DOA0=4 DOA1=4 DOA2=4 DOA3=4 DOA4=4 DOA5=4 DOA6=4 DOA7=4 DOB0=4 DOB1=4 DOB2=4 DOB3=4 DOB4=4 DOB5=4 DOB6=4 DOB7=4 ENA=4 ENB=4 REGCEA=4 REGCEB=4 RSTA=4 RSTB=4 WEA0=4 WEA1=4 WEA2=4 WEA3=4 WEB0=4 WEB1=4 WEB2=4 WEB3=4 | REG_SR CE=786 CK=1288 D=1288 Q=1288 SR=974 SELMUX2_1 0=118 1=118 OUT=118 S0=118 SLICEL A=58 A1=46 A2=73 A3=85 A4=95 A5=105 A6=107 AMUX=39 AQ=31 AX=24 B=78 B1=28 B2=82 B3=106 B4=109 B5=119 B6=119 BMUX=29 BQ=24 BX=20 C=1 C1=23 C2=35 C3=41 C4=121 C5=157 C6=157 CE=63 CIN=34 CLK=143 CMUX=41 COUT=34 CQ=129 CX=136 D1=53 D2=67 D3=143 D4=145 D5=156 D6=157 DMUX=29 DQ=59 DX=14 SR=132 SLICEM A=37 A1=41 A2=41 A3=41 A4=41 A5=41 A6=40 AI=40 AMUX=29 AQ=3 AX=14 B=31 B1=32 B2=33 B3=33 B4=33 B5=34 B6=34 BI=32 BMUX=28 BQ=3 BX=13 C=29 C1=30 C2=30 C3=30 C4=31 C5=32 C6=32 CE=43 CI=30 CIN=1 CLK=43 CMUX=29 COUT=1 CQ=3 CX=15 D=16 D1=33 D2=33 D3=34 D4=34 D5=35 D6=35 DI=32 DMUX=35 DQ=2 DX=30 SR=2 SLICEX A=177 A1=178 A2=244 A3=280 A4=306 A5=329 A6=320 AMUX=65 AQ=371 AX=194 B=154 B1=132 B2=190 B3=218 B4=227 B5=242 B6=237 BMUX=49 BQ=240 BX=123 C=113 C1=118 C2=160 C3=180 C4=191 C5=206 C6=203 CE=266 CLK=465 CMUX=47 CQ=221 CX=99 D=134 D1=106 D2=153 D3=180 D4=187 D5=198 D6=196 DMUX=38 DQ=202 DX=115 SR=352

Software Quality
Run Statistics
Program Name | Runs Started | Runs Finished | Errors | Fatal Errors | Internal Errors | Exceptions | Core Dumps
_compxlibgui | 1 | 1 | 0 | 0 | 0 | 0 | 0
_impact | 6 | 5 | 0 | 0 | 0 | 0 | 0
arwz | 3 | 3 | 0 | 0 | 0 | 0 | 0
bitgen | 69 | 68 | 0 | 0 | 0 | 0 | 0
bitinit | 10 | 10 | 0 | 0 | 0 | 0 | 0
compedklib | 1 | 1 | 0 | 0 | 0 | 0 | 0
compxlib | 1 | 1 | 0 | 0 | 0 | 0 | 0
elfcheck | 18 | 18 | 0 | 0 | 0 | 0 | 0
libgen | 15 | 15 | 0 | 0 | 0 | 0 | 0
map | 78 | 69 | 0 | 0 | 0 | 0 | 0
netgen | 6 | 6 | 0 | 0 | 0 | 0 | 0
ngcbuild | 45 | 45 | 0 | 0 | 0 | 0 | 0
ngdbuild | 134 | 134 | 0 | 0 | 0 | 0 | 0
par | 68 | 68 | 0 | 0 | 0 | 0 | 0
platgen | 11 | 11 | 0 | 0 | 0 | 0 | 0
psf2Edward | 4 | 4 | 0 | 0 | 0 | 0 | 0
trce | 68 | 68 | 0 | 0 | 0 | 0 | 0
xdsgen | 4 | 4 | 0 | 0 | 0 | 0 | 0
xps | 23 | 23 | 0 | 0 | 0 | 0 | 0
xst | 295 | 295 | 0 | 0 | 0 | 0 | 0

Core Statistics
Core Type=MicroBlaze
c_area_optimized=0 | c_avoid_primitives=0 | c_base_vectors=0x00000000 | c_branch_target_cache_size=0
c_cache_byte_size=8192 | c_d_axi=0 | c_d_lmb=1 | c_d_plb=1
c_dcache_always_used=0 | c_dcache_baseaddr=0x00000000 | c_dcache_byte_size=8192 | c_dcache_data_width=0
c_dcache_force_tag_lutram=0 | c_dcache_highaddr=0x3FFFFFFF | c_dcache_line_len=4 | c_dcache_use_writeback=0
c_dcache_victims=0 | c_debug_enabled=1 | c_div_zero_exception=0 | c_dplb_bus_exception=0
c_family=spartan6 | c_fault_tolerant=0 | c_fpu_exception=0 | c_freq=50000000
c_fsl_exception=0 | c_fsl_links=0 | c_i_axi=0 | c_i_lmb=1
c_i_plb=1 | c_icache_always_used=0 | c_icache_baseaddr=0x00000000 | c_icache_data_width=0
c_icache_force_tag_lutram=0 | c_icache_highaddr=0x3FFFFFFF | c_icache_line_len=4 | c_icache_streams=0
c_icache_victims=0 | c_ill_opcode_exception=0 | c_instance=microblaze_0 | c_interconnect=1
c_iplb_bus_exception=0 | c_lockstep_slave=0 | c_m_axi_d_bus_exception=0 | c_m_axi_dc_data_width=32
c_m_axi_dc_exclusive_access=0 | c_m_axi_dp_exclusive_access=0 | c_m_axi_i_bus_exception=0 | c_m_axi_ic_data_width=32
c_mmu_dtlb_size=4 | c_mmu_itlb_size=2 | c_mmu_tlb_access=3 | c_mmu_zones=16
c_number_of_pc_brk=1 | c_number_of_rd_addr_brk=0 | c_number_of_wr_addr_brk=0 | c_opcode_0x0_illegal=0
c_pc_width=32 | c_pvr=0 | c_stream_interconnect=0 | c_unaligned_exceptions=0
c_use_barrel=1 | c_use_branch_target_cache=0 | c_use_dcache=0 | c_use_div=0
c_use_ext_brk=1 | c_use_ext_nm_brk=1 | c_use_extended_fsl_instr=0 | c_use_fpu=0
c_use_hw_mul=1 | c_use_icache=0 | c_use_interrupt=0 | c_use_mmu=0
c_use_msr_instr=1 | c_use_pcmp_instr=1 | c_use_reorder_instr=1 | c_use_stack_protection=0
mb_version=0x1A

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_AND2B1L=1 | NGDBUILD_NUM_BSCAN_SPARTAN6=1 | NGDBUILD_NUM_BUFG=4 | NGDBUILD_NUM_DSP48A1=3
NGDBUILD_NUM_FD=170 | NGDBUILD_NUM_FDC=5 | NGDBUILD_NUM_FDCE=32 | NGDBUILD_NUM_FDC_1=5
NGDBUILD_NUM_FDE=361 | NGDBUILD_NUM_FDE_1=8 | NGDBUILD_NUM_FDP=5 | NGDBUILD_NUM_FDR=917
NGDBUILD_NUM_FDRE=645 | NGDBUILD_NUM_FDRE_1=1 | NGDBUILD_NUM_FDS=25 | NGDBUILD_NUM_FDSE=49
NGDBUILD_NUM_GND=13 | NGDBUILD_NUM_IBUF=3 | NGDBUILD_NUM_INV=25 | NGDBUILD_NUM_LUT1=35
NGDBUILD_NUM_LUT2=136 | NGDBUILD_NUM_LUT3=457 | NGDBUILD_NUM_LUT4=417 | NGDBUILD_NUM_LUT5=308
NGDBUILD_NUM_LUT6=626 | NGDBUILD_NUM_LUT6_2=79 | NGDBUILD_NUM_MULT_AND=2 | NGDBUILD_NUM_MUXCY=72
NGDBUILD_NUM_MUXCY_L=153 | NGDBUILD_NUM_MUXF7=119 | NGDBUILD_NUM_OBUF=8 | NGDBUILD_NUM_PLL_ADV=1
NGDBUILD_NUM_RAM32M=16 | NGDBUILD_NUM_RAMB16BWER=4 | NGDBUILD_NUM_SRL16=1 | NGDBUILD_NUM_SRL16E=34
NGDBUILD_NUM_SRLC16E=88 | NGDBUILD_NUM_VCC=8 | NGDBUILD_NUM_XORCY=110
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_AND2B1L=1 | NGDBUILD_NUM_BSCAN_SPARTAN6=1 | NGDBUILD_NUM_BUFG=4 | NGDBUILD_NUM_DSP48A1=3
NGDBUILD_NUM_FD=170 | NGDBUILD_NUM_FDC=5 | NGDBUILD_NUM_FDCE=32 | NGDBUILD_NUM_FDC_1=5
NGDBUILD_NUM_FDE=361 | NGDBUILD_NUM_FDE_1=8 | NGDBUILD_NUM_FDP=5 | NGDBUILD_NUM_FDR=917
NGDBUILD_NUM_FDRE=645 | NGDBUILD_NUM_FDRE_1=1 | NGDBUILD_NUM_FDS=25 | NGDBUILD_NUM_FDSE=49
NGDBUILD_NUM_GND=13 | NGDBUILD_NUM_IBUF=3 | NGDBUILD_NUM_INV=25 | NGDBUILD_NUM_LUT1=35
NGDBUILD_NUM_LUT2=136 | NGDBUILD_NUM_LUT3=457 | NGDBUILD_NUM_LUT4=417 | NGDBUILD_NUM_LUT5=308
NGDBUILD_NUM_LUT6=626 | NGDBUILD_NUM_LUT6_2=79 | NGDBUILD_NUM_MULT_AND=2 | NGDBUILD_NUM_MUXCY=72
NGDBUILD_NUM_MUXCY_L=153 | NGDBUILD_NUM_MUXF7=119 | NGDBUILD_NUM_OBUF=8 | NGDBUILD_NUM_PLL_ADV=1
NGDBUILD_NUM_PULLUP=8 | NGDBUILD_NUM_RAM32M=16 | NGDBUILD_NUM_RAMB16BWER=4 | NGDBUILD_NUM_SRL16E=35
NGDBUILD_NUM_SRLC16E=88 | NGDBUILD_NUM_TS_TIMESPEC=1 | NGDBUILD_NUM_VCC=8 | NGDBUILD_NUM_XORCY=110

XST Command Line Options
XST_OPTION_SUMMARY
-opt_mode=speed | -netlist_hierarchy=as_optimized | -opt_level=1 | -p=xc6slx9tqg144-3
-top=<design_top> | -ifmt=MIXED | -ifn=<fname>.prj | -ofn=<design_top>
-iobuf=YES | -max_fanout=10000 | -sd=<No customer specific name> | -vlgincdir={"C:\miicroblaze\pcores\" "D:\14.5\ISE_DS\EDK\hw\XilinxBFMinterface\pcores\" "D:\14.5\ISE_DS\EDK\hw\XilinxProcessorIPLib\pcores\" }