Par Statistics
Total Non-vccgnd Signals=2789
Total Non-vccgnd Design Pins=10355
Total Non-vccgnd Conns=10355
Total Non-vccgnd Timing Constrained Conns=9468
Phase 1 CPU=8.3 sec
Phase 2 CPU=9.0 sec
Phase 3 CPU=20.8 sec
Phase 4 CPU=21.7 sec
Phase 5 CPU=31.8 sec
Phase 6 CPU=31.8 sec
Phase 7 CPU=31.8 sec
Phase 8 CPU=31.8 sec
Phase 9 CPU=31.8 sec
Phase 10 CPU=33.0 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=3.5
AvgWirelenPerPin Fanout 3=4.0
AvgWirelenPerPin Fanout 4=4.5
AvgWirelenPerPin Fanout 10=4.3
AvgWirelenPerPin Fanout 50=4.3
AvgWirelenPerPin Fanout 100=14.2
AvgWirelenPerPin Fanout 500=10.3
AvgWirelenPerPin Fanout 5000=1.7
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=10.3484